**Please read the instructions below carefully**

INSTRUCTIONS

1. You may not in any other way than as instructed below add information to this document, or otherwise alter or modify this document.
2. Fill only out the fields indicated in blue.
3. You are required to attach to this form technical documentation from the manufacturer for the item proposed, warranty conditions and the details of the after-sale service conditions

**LOT 1: Servers**

|  |  |
| --- | --- |
| **Confirmation of capacity to provide items/services** | * Supply, deliver and install Two mid-range 2U rack-mounted servers   Place: GFC Head Office in Georgetown |
| ***Declare in the blue field the ability to deliver the required items/services according to the specifications*** |  |

|  |  |
| --- | --- |
| **Product required (Minimum criteria)** | Provide in a separate document a description of the following last 3 years similar experience in:  The supply, delivery and installation of Servers with similar technical specifications with indicative amount and name of client |
| ***Declare in the blue field the ability to deliver the required items/services according to the specifications*** |  |

* 1. Supply, deliver and install Two mid-range 2U rack-mounted servers in the GFC Head Office in Georgetown

|  |  |  |  |
| --- | --- | --- | --- |
| **Item** | Name/reference/code of the product:  Name manufacturer:  (Manufacturer Technical documentation to be annexed to the offer) | | |
| **Technical requirements of the item** | Technical characteristics required | YES/NO  (Declare compliance in blue field) | Technical characteristic of item provided  (Insert in blue field the technical characteristic of the item offered) |
| Chassis | 2U Small-Form-Factor (SFF) |  |  |
| Processors | 2x Intel Xeon, 10 Cores |  |  |
| Memory | 12 x 16Gb Single Rank DIMMs (total 192 Gb) |  |  |
| Storage | 2 x 240Gb Mixed-mode SSD with M.2/NVMe interface |  |  |
| RAID controller | RAID 0,1,5,6,10 |  |  |
| SAN HBA | Dual SAN HBA cards, total 4 x 16Gb FC interfaces |  |  |
| Power | Dual hot-swap Power supply |  |  |
| Management | Advanced management interface, min 5 years subscription |  |  |
| External Interfaces | 4x1Gbps Ethernet |  |  |
| Transceivers | 4 x 16Gb Fibre Channel Transceiver modules |  |  |
| Warranty and Support contract | Minimum 5 years warranty and onsite support, 8x5 NBD |  |  |
| Preferred manufacturer or equivalent | Dell, HPE, IBM, Lenovo |  |  |

|  |  |
| --- | --- |
| **Delivery time/installation plan (timetable)/after sale service** | Provide a maximum 4 pages presentation (in addition to relevant manufacturer technical documentation) of the following in a separate document:   * Rational for proposing the goods and services in response to required technical specifications of this lot * Delivery timetable and installation plan * Proposed service agreement for warranty and maintenance |
| ***Declare in the blue field the ability to deliver according to the timetable*** |  |

**\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**

**Signature**

Representative authorized to sign on behalf of the Tenderer/ Consortium leader, as stated in the identification form